{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["产生单位","处置单位"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"产生单位","index":0,"n_rows":14,"n_cols":9,"rows_kept":14,"merged":[[0,0,0,8]]}
["永达科技2024年危险废弃物产生单位污染环境防治信息公开"]
["序号","废弃物名称","废弃物类别","废物代码","危险特性","产生环节","产生量（吨）","污染预防措施","去向（处置单位）"]
[1,"含油污泥","HW49其他废物","900-047-49","毒性/感染性","污水处理过程",6.82,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽嘉瑞环保科技有限公司/安徽珍昊环保科技有限公司"]
[2,"废油","HW08废矿物油与含矿物油废物","900-249-08","毒性，易燃性","设备检维修过程",6.24,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","合肥市安达新能源有限公司/安徽嘉瑞环保科技有限公司"]
[3,"COD/氨氮废液","HW49其他废物","900-047-49","腐蚀性,反应性,毒性,易燃性","污水在线监测标记过程",0.4,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽嘉瑞环保科技有限公司/安徽珍昊环保科技有限公司"]
[4,"过滤棉","HW49其他废物","900-041-49","毒性/感染性","除尘治理设施过程",0.266,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽嘉瑞环保科技有限公司/安徽珍昊环保科技有限公司"]
[5,"废劳保（含油抹布手套等）","HW49其他废物","900-041-49","毒性/感染性/易燃性","生产过程及设备维护保养过程",0.08,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽珍昊环保科技有限公司"]
[6,"含水废油","HW08废矿物油与含矿物油废物","900-210-08","毒性，易燃性","设备检维修维护保养过程",30.04,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","合肥市安达新能源有限公司"]
[7,"布袋（熔化、浇注）","HW49其他废物","900-041-49","毒性/感染性","除尘治理设施过程",18.44,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽嘉瑞环保科技有限公司/安徽珍昊环保科技有限公司"]
[8,"废活性炭","HW49其他废物","900-039-49","毒性","除尘治理设施过程",15.82,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽嘉瑞环保科技有限公司/安徽珍昊环保科技有限公司"]
[9,"油漆桶","HW49其他废物","900-041-49","感染性,毒性","生产过程及设备地面维护保养过程",12.26,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽嘉鹏特环保科技服务有限公司/安徽嘉瑞环保科技有限公司"]
[10,"三乙胺包装桶","HW49其他废物","900-041-49","感染性,毒性","生产过程",30.29,"于公司危废储存间存放，按危险废物种类进行分区贮存、采用防腐防渗地面、设置导流、收集设施，定期由有资质单位回收处理。","安徽嘉鹏特环保科技服务有限公司/安徽嘉瑞环保科技有限公司"]
[11,"粉尘灰","HW48","321-034-48","反应性、毒性","铝灰热回收铝过程",20.95,"于公司铝灰渣、粉尘灰贮存点存放，定期由有资质单位回收处理。","浙江美臣新材料科技有限公司"]
[12,"铝灰渣","HW48","321-026-48","反应性","再生铝和铝材加工过程",1404.92,"于公司铝灰渣、粉尘灰贮存点存放，定期由有资质单位回收处理。","浙江美臣新材料科技有限公司"]

{"sheet":"处置单位","index":1,"n_rows":22,"n_cols":9,"rows_kept":22,"merged":[[0,0,0,8],[2,0,9,0],[2,1,9,1],[10,0,15,0],[10,1,15,1],[16,0,17,0],[16,1,17,1],[18,0,19,0],[18,1,19,1],[20,0,21,0],[20,1,21,1]]}
["2024年危险废弃物处置单位污染环境防治信息公开"]
["序号","企业名称","废弃物名称","废弃物类别","废物代码","危险特性","处置方式","处置量（吨）","责任人"]
[1,"安徽嘉瑞环保科技有限公司","COD/氨氮废液","HW49其他废物","900-047-49","腐蚀性,反应性,毒性,易燃性","中转、贮存",0.24,"刘晓东"]
[null,null,"废油","HW08废矿物油与含矿物油废物","900-249-08","毒性，易燃性","提炼",5.7,"刘晓东"]
[null,null,"油漆桶","HW49其他废物","900-041-49","感染性,毒性","中转、贮存",1.43,"刘晓东"]
[null,null,"三乙胺包装桶","HW49其他废物","900-041-49","感染性,毒性","中转、贮存",2.97,"刘晓东"]
[null,null,"废活性炭","HW49其他废物","900-039-49","毒性","中转、贮存",11.44,"刘晓东"]
[null,null,"布袋（熔化、浇注）","HW49其他废物","900-041-49","毒性/感染性","中转、贮存",16.57,"刘晓东"]
[null,null,"过滤棉","HW49其他废物","900-041-49","毒性/感染性","中转、贮存",0.15,"刘晓东"]
[null,null,"含油污泥","HW49其他废物","900-047-49","毒性/感染性","中转、贮存",3.99,"刘晓东"]
[2,"安徽珍昊环保科技有限公司","废劳保（含油抹布手套等）","HW49其他废物","900-041-49","毒性/感染性/易燃性","焚烧",0.08,"方祖波"]
[null,null,"废活性炭","HW49其他废物","900-039-49","毒性","焚烧",4.38,"方祖波"]
[null,null,"布袋（熔化、浇注）","HW49其他废物","900-041-49","毒性/感染性","焚烧",1.73,"方祖波"]
[null,null,"过滤棉","HW49其他废物","900-041-49","毒性/感染性","焚烧",0.116,"方祖波"]
[null,null,"COD/氨氮废液","HW49其他废物","900-047-49","腐蚀性,反应性,毒性,易燃性","焚烧",0.18,"方祖波"]
[null,null,"含油污泥","HW49其他废物","900-047-49","毒性/感染性","焚烧",2.83,"方祖波"]
[3,"合肥市安达新能源有限公司","废油","HW08废矿物油与含矿物油废物","900-249-08","毒性，易燃性","提炼",0.54,"万家文"]
[null,null,"含水废油","HW08废矿物油与含矿物油废物","900-210-08","毒性，易燃性","提炼",30.04,"万家文"]
[4,"安徽嘉鹏特环保科技服务有限公司","油漆桶","HW49其他废物","900-041-49","感染性,毒性","清洗、利用",10.83,"澎湃"]
[null,null,"三乙胺包装桶","HW49其他废物","900-041-49","感染性,毒性","清洗、利用",27.918,"澎湃"]
[5,"浙江美臣新材料科技有限公司","粉尘灰","HW48","321-034-48","反应性、毒性","提炼、循环利用",20.95,"朱剑帆"]
[null,null,"铝灰渣","HW48","321-026-48","反应性","提炼、循环利用",1393.99,"朱剑帆"]